{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279875403316"]
[null,null,"Titolo",null,"ANSI C63.4-2014 (Revision of ANSI C63.4-2009) - Redline : American National Standard for Methods of Measurement of Radio-Noise Emissions from Low-Voltage Electrical and Electronic Equipment in the Range of 9 kHz to 40 GHz - Redline / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, New Jersey : , : IEEE, , 2014"]
[null,null,"ISBN",null,"1-5044-0133-6"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"621.38224"]
[null,null,"Soggetti",null,"Electric apparatus and appliances - Testing"]
[{"$nulls":4},"Noise - Measurement - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","ANSI C63.4, conducted emission testing, conducting ground plane, digital equipment, electric field measurement, line impedance stabilization network, low-voltage electrical equipment, low-voltage electronic equipment, magnetic field measurement, normalized site attenuation, radiated emission testing, radio-noise emissions, radio-noise power, site attenuation, unintentional radiators."]