{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[11,2,11,3],[12,2,12,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279876803316"]
[null,null,"Titolo",null,"ANSI/IEEE Std 1122-1987 : IEEE Standard for Digital Recorders for Measurements in High-Voltage Impulse Tests / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 1988"]
[null,null,"ISBN",null,"0-7381-4143-7"]
[null,null,"Descrizione fisica",null,"1 online resource (20 pages)"]
[null,null,"Disciplina",null,"621.381"]
[null,null,"Soggetti",null,"Digital electronics"]
[{"$nulls":4},"Oscilloscopes"]
[{"$nulls":4},"Electric apparatus and appliances - Testing - Standards"]
[{"$nulls":4},"High voltages - Measurement"]
[{"$nulls":4},"Standards, Engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Digital recorders and digital oscilloscopes used for measurements during tests with high-impulse voltages and high-impulse currents are considered. Terms specifically related to the digital recorders used for monitoring high-voltage and high-current impulse tests are defined. The performance characteristics for such recorders, necessary to ensure their compliance with the requirements for high-voltage and for high-current impulse tests, are specified. The tests and procedures that are necessary to show that these performance characteristics are within those specified limits are indicated."]