{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280193803316"]
[null,null,"Titolo",null,"IEEE standard for low-rate wireless networks . Amendment 3 Use of the 865 MHz to 867 MHz band in India"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2017"]
[null,null,"ISBN",null,"1-5044-2320-8"]
[null,null,"Descrizione fisica",null,"1 online resource (201 pages)"]
[null,null,"Disciplina",null,"004.68"]
[null,null,"Soggetti",null,"Local area networks (Computer networks) - Standards"]
[{"$nulls":4},"Metropolitan area networks (Computer networks) - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","A physical (PHY) layer enabling the use of the 865 MHz to 867 MHz band in India is defined in this amendment. The supported data rate should be at least 40 kb/s and the typical line-of-sight range should be on the order of 5 km using an omnidirectional antenna. Included are any channel access and/or timing changes in the medium access control necessary to support this PHY layer."]