{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280417103316"]
[null,null,"Titolo",null,"IEEE Std 802.3x-1997 and IEEE Std 802.3y-1997 (Supplement to ISO/IEC 8802-3: 1996; ANSI/IEEE Std 802.3, 1996 Edition) : IEEE Standards for Local and Metropolitan Area Networks: Supplements to Carrier Sense Multiple Access With Collision Detection (CSMA/CD) / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 1997"]
[null,null,"ISBN",null,"0-7381-0277-6"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"004.67"]
[null,null,"Soggetti",null,"Metropolitan area networks (Computer networks)"]
[{"$nulls":4},"Local area networks (Computer networks)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Superseded by IEEE Std 802.3-2002 Necessary changes and additions are made to provide for an additional, full duplex mode of operation on a speed-independent basis. Changes are made to the MAC and selected Physical Layer implementations (10BASE-T, 10BASE-FL, 100BASE-T) to support full duplex. A mechanism for pause-based flow control is also added.p> Abstract 802.3y: Changes and additions to the 100BASE-T portion of IEEE Std 802.3 are provided to specify an additional 100 Mb/s transceiver type 100BASE-T, which can support full duplex operation over two pairs of Category 3 or better cabling."]