{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280423603316"]
[null,null,"Titolo",null,"IEEE Standard for Information Technology : Telecommunications and information exchange between systems - Local and Metropolitan Area Networks - Part 3: Carrier Sense Multiple Access with Collision Detection (CSMA/CD) Access Method and Physical Layer Specifications - Physical Layer Parameters and Specifications for 1000 Mb/s Operation over 4 pair of Category 5 Balanced Copper Cabling, Type 1000BASE-T / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, USA : , : IEEE, , 1999"]
[null,null,"ISBN",null,"0-7381-3765-0"]
[null,null,"Descrizione fisica",null,"1 online resource (143 pages)"]
[null,null,"Disciplina",null,"004"]
[null,null,"Soggetti",null,"Information technology"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Superseded by IEEE Std 802.3-2002. This IEEE Standards product is part of the 802 Family on LAN/MAN. Abstract: Type 1000BASE-T PCS, type 1000BASE-T PMA sublayer, and type 1000BASE-T Medium Dependent Interface (MDI) are defined. This supplement provides fully functional, electrical and mechanical specifications for the type 1000BASE-T PCS, PMA, and MDI. This supplement also specifies the baseband medium used with 1000BASE-T."]