{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[13,2,13,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280500803316"]
[null,null,"Titolo",null,"1999 IEEE Recommended Practice for Installation and Maintenance of Nicel-Cadmium Batteries for Photovoltaic (PV) Systems"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified], : IEEE, 2000"]
[null,null,"ISBN",null,"0-7381-2200-9"]
[null,null,"Descrizione fisica",null,"1 online resource (v, 12 pages)"]
[null,null,"Collana",null,"IEEE Std ; ; Volume 1145"]
[null,null,"Disciplina",null,"621.314"]
[null,null,"Soggetti",null,"Electrical engineering - standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"References -- Citations -- Keywords -- Metrics -- Versions."]
[null,null,null,"Sommario/riassunto","Safety precautions, installation design considerations, and procedures for receiving, storing, commissioning, and maintaining pocket- and fiber-plate nickel-cadmium storage batteries for photovoltaic (PV) power systems are provided. Disposal and recycling recommendations are also discussed. This recommended practice applies to all PV power systems, regardless of size or application, that contain nickel-cadmium battery storage subsystems."]