{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280640603316"]
[null,null,"Titolo",null,"IEEE Std C37.71-2001 : IEEE Standard for Three-Phase, Manually Operated Subsurface and Vault Load-Interrupting Switches for Alternating-Current Systems / / Institute of Electrical and Electronics Engineers (IEEE)"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : Institute of Electrical and Electronics Engineers (IEEE), , 2001"]
[null,null,"ISBN",null,"0-7381-2841-4"]
[null,null,"Descrizione fisica",null,"1 online resource (vi, 23 pages) : illustrations"]
[null,null,"Disciplina",null,"621.31923"]
[null,null,"Soggetti",null,"Underground electric lines"]
[{"$nulls":4},"Electric switchgear - Standards"]
[{"$nulls":4},"Standards, Engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","\"Requirements are given for three-phase group operated subsurface and vault load-interrupting switchgear with maximum ratings of 600 A and 38 kV, and for utilizing separable insulated connectors. definitions are given, and service conditions and ratings are discussed. Design tests, production tests, and construction requirements are included.\"."]