{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996280813003316"]
[null,null,"Autore",null,"Institute of Electrical and Electronics Engineers"]
[null,null,"Titolo",null,"ANSI/IEEE Std 11-1980 (Revision of IEEE Std 11-1962): : IEEE Standard for Rotating Electric Machinery for Rail and Road Vehicles / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York, USA : , : IEEE, , 1981"]
[null,null,"ISBN",null,"0-7381-0761-1"]
[null,null,"Descrizione fisica",null,"1 online resource (39 pages)"]
[null,null,"Disciplina",null,"621.310420218"]
[null,null,"Soggetti",null,"Electric machinery - Standards"]
[{"$nulls":4},"Electric generators - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard applies to rotating electric machinery which forms part of the propulsion and major auxiliary equipment on internally and externally powered electrically propelled rail and road vehicles and similar large transport and haulage vehicles and their trailers where speciÞed in the contract. Major auxiliary equipment includes equipment such as blower and compressor motors, motor-generator and motoralternator sets, auxiliary generators, and exciters, usually larger than 3 kilowatts."]