{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996281049103316"]
[null,null,"Titolo",null,"IEEE Std C37.30.1-2011 : IEEE Standard Requirements for AC High-Voltage Air Switches Rated Above 1000 V / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2012"]
[null,null,"ISBN",null,"0-7381-7157-3"]
[null,null,"Descrizione fisica",null,"1 online resource (ix, 92 pages)"]
[null,null,"Disciplina",null,"621.3028"]
[null,null,"Soggetti",null,"High voltages - Testing"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Required ratings, construction requirements, design test requirements, applications, and suggested practices for all high-voltage enclosed indoor and outdoor and nonenclosed indoor and outdoor switches rated above 1000 V are specified. This includes ratings and requirements for such switches as disconnecting, selector, horn-gap, and grounding for manual and power operation, except for interrupter switches, distribution-enclosed single-pole air switches, and distribution cutouts fitted with disconnecting blades. Keywords: high-voltage switches, IEEE C37.30.1, indoor switches, outdoor switches."]