{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[14,2,14,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996483071403316"]
[null,null,"Autore",null,"Ružbarský Juraj"]
[null,null,"Titolo",null,"Contactless system for measurement and evaluation of machined surfaces / / Juraj Ružbarský"]
[null,null,"Pubbl/distr/stampa",null,"Cham, Switzerland : , : Springer, , [2022]"]
[{"$nulls":4},"©2022"]
[null,null,"ISBN",null,"9783031089817"]
[{"$nulls":4},"9783031089800"]
[null,null,"Descrizione fisica",null,"1 online resource (105 pages)"]
[null,null,"Collana",null,"SpringerBriefs in Applied Sciences and Technology"]
[null,null,"Disciplina",null,"658.5"]
[null,null,"Soggetti",null,"Industrial management"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,"Nota di contenuto",null,"Intro -- Preface -- Introduction -- Contents -- Symbols and Abbreviations -- 1 Current State of the Art -- 1.1 Surface Roughness -- 1.2 Machined Surface Characteristics -- 1.2.1 Quality of Machined Surface Area -- 1.2.2 Theoretical and Actual Surface Roughness -- 1.2.3 Geometric Surface Waviness -- 1.3 Quality Parameters -- 1.3.1 Evaluation of Surface Character -- 1.4 Measurement of Machined Surface Roughness -- 1.4.1 Roughness Measurement Methods -- 1.4.2 Roughness Measurement Devices and Methods -- 1.5 Contact Methods of Roughness Measurement -- 1.5.1 Measruement System MAHR MarSurf PS1 -- 1.5.2 Measuring Instrument CarlZeiss Handysurf E-35A -- 1.6 Contactless Methods of Roughness Measurement -- 1.6.1 Measurement by Laser Sensor -- 1.6.2 Measurement System MAHR MarSurf WS 1 -- 1.6.3 Measuring Instrument Taylor Hobson CCI HD -- 1.7 Laser Profilometry LPM -- 1.7.1 Laser -- 1.7.2 Laser Light Color and Performance -- 1.8 Basic Components of Experimental Set-Ups of Optical 3D Methods -- 1.8.1 Point and Linear Optical Structures -- 1.8.2 Planar Optical Structures -- 1.8.3 Intensity Optical Structures -- 1.8.4 Applied Optical Detectors -- 1.8.5 CCD Detectors -- 1.8.6 CMOS Detectors -- 1.9 Overview of Applied 3D Methods -- 1.9.1 Laser Triangulation -- 1.9.2 Fourier Profilometry -- 1.9.3 Phase Shifting Profilometry -- 1.9.4 Phase Measuring Deflectometry -- 1.9.5 Moiré Topography -- 1.9.6 White Light Interferometry -- 1.9.7 Fizeau Interferometry -- 1.10 Comparison of Parameters of Equipment Applied in Surface Roughness Measurement -- References -- 2 Laser Profilometer Design -- 2.1 "]
[{"$nulls":4},"Frame Structure -- 2.2 Micrometric Slide -- 2.3 Objective -- 2.4 CMOS Camera -- 2.5 Applied Laser -- 2.6 Lighting -- 2.7 LPM View Software -- 2.8 General Characteristics of the LPM System -- References -- 3 Production of Experimental Samples."]
[{"$nulls":4},"3.1 Material Characteristics of Proposed Samples -- 3.2 Production of Samples by AWJ Technology -- References -- 4 Description of Measuring Experiment -- 4.1 Measurement of Selected Roughness Parameters by Contact Method -- 4.2 Measurement of Selected Roughness Parameters by Contactless Method -- 5 Measurement of Roughness Parameters by Contact Surface Roughness Tester -- 5.1 Samples with Declared Roughness of Ra = 6.3 μm (AL120, SS050, FS050) -- 5.2 Samples with Declared Roughness of Ra = 12.5 μm (AL220, SS120, FS100) -- 5.3 Samples with Declared Roughness of Ra = 25 μm (AL370, SS150, FS150) -- 6 Measurement of Roughness Parameters by Contactless Laser Profilometer LPM -- 6.1 Samples with Declared Roughness of Ra = 6.3 μm (AL120, SS050, FS050) -- 6.2 Samples with Declared Roughness of Ra = 12.5 μm (AL220, SS120, FS100) -- 6.3 Samples with Declared Roughness of Ra = 25 μm (AL370, SS150, FS150) -- 7 Glossy Surface Measurement -- 7.1 Comparison of Achieved Results by Contact and Contactless Roughness Surface Testers -- Reference -- 8 Conclusion -- Uncited References."]