{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996551163003316"]
[null,null,"Titolo",null,"C37.98-2023 - IEEE Standard for Seismic Qualification Testing of Protective Relays and Auxiliaries for Nuclear Facilities / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , [2023]"]
[{"$nulls":4},"©2023"]
[null,null,"ISBN",null,"1-5044-9880-1"]
[null,null,"Descrizione fisica",null,"1 online resource (34 pages)"]
[null,null,"Disciplina",null,"333.7924"]
[null,null,"Soggetti",null,"Nuclear energy"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The methods and conditions for seismic qualification of protective relays and auxiliaries such as test and control switches, terminal blocks, and indicating lamps for use in nuclear facilities are described in this standard. The primary intent of this standard is to focus on fragility testing and seismic qualification, also known as proof testing (either to generic levels or specific levels). Relays used in nuclear facilities are covered in this standard, but it may also be applied to any area in which the seismic response of relays is a design consideration. The prerequisites for the seismic test are defined in IEEE Std C37.105™."]