{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[18,2,18,3],[19,2,19,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910172596403321"]
[null,null,"Titolo",null,"IEEE Std C37.13.1-2016 (Revision of IEEE Std C37.13.1-2006) : IEEE Standard for Definite-Purpose Switching Devices for Use in Metal-Enclosed Low-Voltage (600 V AC and Below) Power Circuit Breaker Switchgear / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2017"]
[null,null,"ISBN",null,"1-5044-2276-7"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"621.317"]
[null,null,"Soggetti",null,"Electric circuit-breakers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Definite-purpose switching devices for use in metal-enclosed low-voltage power circuit breaker switchgear are covered in this standard. The switching devices are fused, drawout type, three-pole construction, with one or more rated maximum ac voltages of 600 V, 508 V, and 254 V for application on systems having nominal ac voltages of 600 V, 480 V, and 240 V. The switching devices are power operated with integral or separately mounted overcurrent protective devices. Service conditions, ratings, functional components, temperature limitations and classifications of insulating materials, insulation (dielectric) withstand voltage requirements, test procedures, and application are addressed in this standard. The switching devices are normally used in applications that require frequency of operation greater than normal operations expected of low-voltage power circuit breakers."]
[null,"2.","Record Nr.",null,"UNISA996564470903316"]
[null,null,"Titolo",null,"IEEE/IFIP ... International Conference on VLSI and System-on-Chip : [proceedings]"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, NJ, : Institute of Electrical and Electronics Engineers"]
[null,null,"ISSN",null,"2324-8440"]
[null,null,"Disciplina",null,"621.3815"]
[null,null,"Soggetti",null,"Integrated circuits - Very large scale integration"]
[{"$nulls":4},"Conference papers and proceedings."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Periodico"]