{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996574833803316"]
[null,null,"Titolo",null,"400.5-2021 - IEEE Guide for Field Testing of DC Shielded Power Cable Systems Rated 5 kV and Above with High Direct Current Test Voltages / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 2022"]
[null,null,"ISBN",null,"1-5044-8281-6"]
[null,null,"Descrizione fisica",null,"1 online resource (25 pages)"]
[null,null,"Disciplina",null,"624.1774"]
[null,null,"Soggetti",null,"Cable"]
[{"$nulls":4},"Cables structures"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The recommended practices and procedures for direct voltage acceptance and maintenance testing of shielded, insulated power cable systems rated 5 kV and above for dc service are presented in this guide. It applies to all types of power cable systems used for transmission of dc voltages and can include laminated or extruded cables designed for dc service. The tabulated test levels assume that the cable systems have an effectively grounded neutral system or a grounded metallic shield."]