{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996574962603316"]
[null,null,"Titolo",null,"1407-2021 - IEEE Guide for Accelerated Aging Tests for 5 kV to 46 kV Extruded Electric Power Cables Using Water-Filled Tanks / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 2022"]
[null,null,"ISBN",null,"1-5044-8163-1"]
[null,null,"Descrizione fisica",null,"1 online resource (53 pages)"]
[null,null,"Disciplina",null,"536.5"]
[null,null,"Soggetti",null,"Temperature"]
[{"$nulls":4},"Temperature measurements"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Provided in this guide are information and recommendations on the equipment, cable specimens, test conditions, test control methodologies, measurements, data analysis, and interpretation in performing accelerated aging tests for 5 kV to 46 kV rated cables using water-filled tanks. The accelerated aging tests may be time-to-failure tests and/or tests in which the samples are aged for fixed times followed by diagnostic testing."]