{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996577946103316"]
[null,null,"Titolo",null,"IEEE Std 572-2019 (Revision of IEEE Std 572-2006) : IEEE standard for qualification of class 1E connection assemblies for nuclear power generating stations and other nuclear facilities / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, New York : , : IEEE, , 2019"]
[null,null,"ISBN",null,"1-5044-5604-1"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Collana",null,"IEEE Std ; ; 572-2019"]
[null,null,"Disciplina",null,"621.48"]
[null,null,"Soggetti",null,"Nuclear power plants"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Basic requirements, direction, and methods for qualifying Class lE connection assemblies for service in nuclear power generating stations and other nuclear facilities are provided in this standard. These requirements include connectors, terminations, and environmental seals in combination with related cables or wires as assemblies. Qualification of cable with connectors to this standard does not replace qualification to IEEE Std 383(TM)-2015. This standard does not apply to containment electric penetrations, fire stops, in-line splices, components for service within the reactor vessel, or fiber optic connectors. (Refer to IEEE Std 1682(TM)-2011.) The qualification requirements in this standard, when met, demonstrate and document the ability of the equipment to perform safety function(s) under applicable service conditions (including design basis events) reducing the risks of common cause equipment failures. This standard does not provide environmental stress levels and performance requirements."]