{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[19,2,19,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135783003321"]
[null,null,"Titolo",null,"ANSI N42.25-1997 : American National Standard Calibration and Usage of Alpha/Beta Proportional Counters / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, New Jersey : , : IEEE, , 1997"]
[null,null,"ISBN",null,"0-7381-0749-2"]
[null,null,"Descrizione fisica",null,"1 online resource (32 pages)"]
[null,null,"Disciplina",null,"621.372"]
[null,null,"Soggetti",null,"Calibration - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard establishes methods for the calibration and use of gas proportional counters with and without active guard detectors. This standard also establishes methods for measuring the alpha and beta counting plateau, crosstalk factors, background, alpha and beta efficiency from prepared standards, correction factors for samples whose self-attenuation or mass differs from that of the standard, and calculation of the sample activities together with their random and total uncertainties. Correction for pulse pileup due to high count rate is also discussed. Although many principles articulated in this standard apply to the counting of radionuclides emitting a maximum beta energy below 100 keV as well, the counting of these low-energy beta emitters requires a higher degree of attention to detail in sample preparation, instrument calibration, and measurement correction factors than addressed in this standard. Therefore, this standard is intended for measuring radionuclides with maximum beta energies above 100 keV."]
[null,"2.","Record Nr.",null,"UNISA996581541903316"]
[null,null,"Titolo",null,"Proceedings  / / UKSim European Symposium on Computer Modeling and Simulation"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, NJ : , : IEEE"]
[null,null,"ISSN",null,"2473-3539"]
[null,null,"Disciplina",null,"003"]
[null,null,"Soggetti",null,"Computer simulation"]
[{"$nulls":4},"Periodicals."]
[{"$nulls":4},"Conference papers and proceedings."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Periodico"]