{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[18,2,18,3],[19,2,19,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA990000111620403321"]
[null,null,"Autore",null,"Varriale, Vincenzo"]
[null,null,"Titolo",null,"Nuove formole pel calcolo del lavoro dei mulini a ritrecine : utili ai periti destinati a determinare la quota fissa di tassa sulla macinazione dei cereali / Vincenzo Varriale"]
[null,null,"Pubbl/distr/stampa",null,"Napoli, : Stabilimento tipografico, 1874"]
[null,null,"Descrizione fisica",null,"64 p., 1 c. di tav. : ill. ; 24 cm"]
[null,null,"Disciplina",null,"690.54"]
[null,null,"Locazione",null,"FINBC"]
[null,null,"Collocazione",null,"13 AR 23 C 35"]
[null,null,"Lingua di pubblicazione",null,"Italiano"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,"2.","Record Nr.",null,"UNINA9910688471203321"]
[null,null,"Titolo",null,"Geopolymers and Other Geosynthetics / / edited by Mazen Alshaaer and Han-Yong Jeon"]
[null,null,"Pubbl/distr/stampa",null,"London : , : IntechOpen, , 2020"]
[null,null,"Descrizione fisica",null,"1 online resource (180 pages) : illustrations"]
[null,null,"Disciplina",null,"624.18923"]
[null,null,"Soggetti",null,"Geosynthetics"]
[{"$nulls":4},"Inorganic polymers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","Geopolymers are applied to material classes that are chemically transformed from low crystallinity aluminusilicates to three-dimensional inorganic polymers (tectosilicates). The resulting material has properties similar to natural minerals, so it is called artificial rock. However, these materials exhibit a chemical composition and mineralogical structure similar to feldspar, feldspathoidal, and zeolites consisting of a polymeric Si-O- Al framework, with a microcrystalline or an amorphous structure. Although geopolymers have attractive engineering and environmental characteristics, there are some challenges in commercializing these materials. In this book, these challenges will be addressed along with introducing the functional geopolymers as an effective approach to commercializing these materials and making them economically feasible."]