{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135283403321"]
[null,null,"Titolo",null,"ANSI C63.18-2014 (Revision of ANSI C63.18-1997) : American National Standard Recommended Practice for an On-Site, Ad Hoc Test Method for Estimating Electromagnetic Immunity of Medical Devices to Radiated Radio-Frequency (RF) Emissions from RF Transmitters / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, NY, USA : , : IEEE, , 2014"]
[null,null,"ISBN",null,"0-7381-9160-4"]
[null,null,"Descrizione fisica",null,"1 online resource (xi, 50 pages) : illustrations"]
[null,null,"Collana",null,"IEEE Std"]
[null,null,"Disciplina",null,"681.761"]
[null,null,"Soggetti",null,"Medical instruments and apparatus"]
[{"$nulls":4},"Electromagnetic compatibility"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","A guide to evaluating electromagnetic immunity of medical devices against radiated radio-frequency (RF) emissions from common RF transmitters is provided in this recommended practice (e.g., two-way radios; walkie-talkies; mobile phones; wireless-enabled tablets, e-readers, laptop computers, and similar devices; RFID readers; networked mp3 players; two-way pagers; and wireless personal digital assistants [PDAs]). A comprehensive test or a guarantee is not provided by this protocol but, instead, a basic evaluation is given that can help identify medical devices that might be particularly vulnerable to interference from common RF transmitters."]