{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910147227103321"]
[null,null,"Titolo",null,"IEEE Std 1532-2002 (Revision of IEEE Std 1532-2001) : IEEE Standard for In-System Configuration of Programmable Devices / / Institute of Electrical and Electronics Engineers (IEEE)"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : Institute of Electrical and Electronics Engineers (IEEE), , 2003"]
[null,null,"ISBN",null,"0-7381-3508-9"]
[null,null,"Descrizione fisica",null,"1 online resource (vii, 141 pages) : illustrations"]
[null,null,"Disciplina",null,"690.0218"]
[null,null,"Soggetti",null,"Standards, Engineering"]
[{"$nulls":4},"Programmable logic devices - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","\"The communication protocol described by IEEE Std 1149.1 (Standard Test Access Port and Boundary-Scan Architecture) has been adopted by this standard for providing standardized programming access and methodology for programmable integrated circuit devices. Devices that implement this standard shall first be compliant with IEEE 1149.1 used for testing purposes. A device, or set of devices, implementing this standard may be programmed (written), read back, erased, and verified, singly or concurrently, with a standardized set of resources. Sample implementation and application details (which are not part of this standard) are included for illustrative purposes.\"."]