{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[22,2,22,3],[23,2,23,3],[26,2,26,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910254174203321"]
[null,null,"Autore",null,"Schirru Michele"]
[null,null,"Titolo",null,"Development of an Ultrasonic Sensing Technique to Measure Lubricant Viscosity in Engine Journal Bearing In-Situ / / by Michele Schirru"]
[null,null,"Pubbl/distr/stampa",null,"Cham : , : Springer International Publishing : , : Imprint : Springer, , 2017"]
[null,null,"ISBN",null,"9783319534084"]
[null,null,"Edizione",null,"[1st ed. 2017.]"]
[null,null,"Descrizione fisica",null,"1 online resource (XVI, 167 p. 155 illus., 80 illus. in color.)"]
[null,null,"Collana",null,"Springer Theses, Recognizing Outstanding Ph.D. Research, , 2190-5053"]
[null,null,"Disciplina",null,"620.11274"]
[null,null,"Soggetti",null,"Acoustical engineering"]
[{"$nulls":4},"Tribology"]
[{"$nulls":4},"Corrosion and anti-corrosives"]
[{"$nulls":4},"Coatings"]
[{"$nulls":4},"Automotive engineering"]
[{"$nulls":4},"Materials science"]
[{"$nulls":4},"Materials—Surfaces"]
[{"$nulls":4},"Thin films"]
[{"$nulls":4},"Engineering Acoustics"]
[{"$nulls":4},"Tribology, Corrosion and Coatings"]
[{"$nulls":4},"Automotive Engineering"]
[{"$nulls":4},"Characterization and Evaluation of Materials"]
[{"$nulls":4},"Surfaces and Interfaces, Thin Films"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references at the end of each chapters."]
[null,null,"Nota di contenuto",null,"Introduction -- Background on Viscosity and Lubrication -- Background on Ultrasound -- Literature review -- A Novel Ultrasonic Model for Non-Newtonian Fluids -- Viscosity Measurement at an Aluminium-Oil Boundary -- The Matching Layer Method -- Viscosity Measurement in a Journal Bearing -- Conclusions."]
[null,null,null,"Sommario/riassunto","This thesis presents a novel ultrasonic instrument for non-invasive and in-situ characterization of journal bearing lubricant viscosity. In particular, the application to journal bearings is described by non-invasively measuring the viscosity and localized power losses throughout operation. This ultrasonic viscometer is based on the reflection of polarized shear waves from a thin resonating coating layer "]
[{"$nulls":4},"to increase the measurement sensitivity, in comparison to conventional ultrasonic methods. This instrument allows for a full engine oil viscoelastic characterization in-situ. The book investigates the effects of temperature, pressure and shear rate, and describes in detail the ultrasonic setup and method. Further, it demonstrates that the same technique can be applied similarly to monitor the lubrication of other engine components. As such, it offers a unique instrument that can drive the research of oil formulations to improve engine performance and fulfill the requirements of international fuel economy regulations. ."]