{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[19,2,19,3],[20,2,20,3],[23,2,23,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910254358603321"]
[null,null,"Titolo",null,"Applications to Marine Disaster Prevention : Spilled Oil and Gas Tracking Buoy System / / edited by Naomi Kato"]
[null,null,"Pubbl/distr/stampa",null,"Tokyo : , : Springer Japan : , : Imprint : Springer, , 2017"]
[null,null,"ISBN",null,"4-431-55991-4"]
[null,null,"Edizione",null,"[1st ed. 2017.]"]
[null,null,"Descrizione fisica",null,"1 online resource (207 p.)"]
[null,null,"Disciplina",null,"620"]
[null,null,"Soggetti",null,"Ocean engineering"]
[{"$nulls":4},"Robotics"]
[{"$nulls":4},"Automation"]
[{"$nulls":4},"Oceanography"]
[{"$nulls":4},"Quality control"]
[{"$nulls":4},"Reliability"]
[{"$nulls":4},"Industrial safety"]
[{"$nulls":4},"Water - Pollution"]
[{"$nulls":4},"Offshore Engineering"]
[{"$nulls":4},"Robotics and Automation"]
[{"$nulls":4},"Quality Control, Reliability, Safety and Risk"]
[{"$nulls":4},"Waste Water Technology / Water Pollution Control / Water Management / Aquatic Pollution"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,"Nota di contenuto",null,"Introduction -- Lessons from Marine-Based Oil Spill and Gas Leak Accidents -- Development and Operation of Underwater Robot for Autonomous Tracking and Monitoring of Subsea Plumes after Oil Spill and Gas Leak from Seabed, and Analyses of Measured Data -- Development of a Robotic Floating Buoy for Autonomously Tracking Oil Slicks Drifting on the Sea Surface (SOTAB-II): Experimental Results -- Numerical Simulation of Oil and Gas Blowout from Seabed in Deep Water -- Effect of liquid-gas interaction on plume structure in blowout flow -- Numerical simulation of spilled oil drifting with data assimilation -- Conclusions."]
[null,null,null,"Sommario/riassunto","This book focuses on the recent results of the research project funded by a Grant-in-Aid for Scientific Research (S) of the Japan Society for the Promotion of Science (No. 23226017) from FY 2011 to FY 2015 on an "]
[{"$nulls":4},"autonomous spilled oil and gas tracking buoy system and its applications to marine disaster prevention systems from a scientific point of view. This book spotlights research on marine disaster prevention systems related to incidents involving oil tankers and offshore platforms, approaching these problems from new scientific and technological perspectives. The most essential aspect of this book is the development of a deep-sea underwater robot for real-time monitoring of blowout behavior of oil and gas from the seabed and of a new type of autonomous surface vehicle for real-time tracking and monitoring of oil spill spread and drift on the sea surface using an oil sensor. The mission of these robots is to provide the simulation models for gas and oil blowouts or spilled oil drifting on the sea surface with measured data for more precision of predictions of oil and gas behavior. ."]