{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[17,2,17,3],[18,2,18,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910298590603321"]
[null,null,"Autore",null,"Zope Indraneel Suhas"]
[null,null,"Titolo",null,"Fire Retardancy Behavior of Polymer/Clay Nanocomposites / / by Indraneel Suhas Zope"]
[null,null,"Pubbl/distr/stampa",null,"Singapore : , : Springer Singapore : , : Imprint : Springer, , 2018"]
[null,null,"ISBN",null,"981-10-8327-4"]
[null,null,"Edizione",null,"[1st ed. 2018.]"]
[null,null,"Descrizione fisica",null,"1 online resource (190 pages)"]
[null,null,"Collana",null,"Springer Theses, Recognizing Outstanding Ph.D. Research, , 2190-5053"]
[null,null,"Disciplina",null,"628.9223"]
[null,null,"Soggetti",null,"Ceramics"]
[{"$nulls":4},"Glass"]
[{"$nulls":4},"Composite materials"]
[{"$nulls":4},"Engineering—Materials"]
[{"$nulls":4},"Polymers"]
[{"$nulls":4},"Ceramics, Glass, Composites, Natural Materials"]
[{"$nulls":4},"Materials Engineering"]
[{"$nulls":4},"Polymer Sciences"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,"Nota di contenuto",null,"Introduction -- Literature Review -- Experimental Methodology -- Decomposition Behavior of Metal-ion Exchanged Clay -- Thermo-oxidative Decomposition Behavior of Polyamide 6 Nanocomposites with Metal-ion Exchanged Clays -- Thermo-oxidative Decomposition Behavior of Polyamide 6 Nanocomposites with Structurally Different Clays -- Controlling the Interfacial Interactions Between Clay and Host Polyamide 6 Matrix -- Clay Catalysis and Fire Retardancy of Polymer/Clay Nanocomposites: A Complete Overview."]
[null,null,null,"Sommario/riassunto","This thesis investigates the early ignition behavior of polymer/clay nanocomposites, which are perceived as potential eco-friendly flame retardant systems. It examines the correlation between clay structural chemistry and high-temperature transformations with clay-assisted decomposition of organic macromolecules. In particular, it investigates the unique effects of metal ions like Mg2+, Al3+ and Fe3+ that are inherent in clays (smectite) on the combustion and thermo-oxidative decomposition of polyamide 6. The results indicate that metal ions present on/in montmorillonite platelets have preferential reactivity towards peroxy/alkoxy groups during polyamide 6 thermal "]
[{"$nulls":4},"decomposition.  Lastly, a simple solution in the form of a physical coating on clay surface is proposed, based on the role of polymer–clay interfacial interaction."]