{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[10,2,10,3],[12,2,12,3],[13,2,13,3],[17,2,17,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910299474403321"]
[null,null,"Titolo",null,"Robotic sailing 2013 : proceedings of the 6th International Robotic Sailing Conference / / [edited by] Fabrice Le Bars, Luc Jaulin"]
[null,null,"Pubbl/distr/stampa",null,"New York, : Springer, 2013"]
[null,null,"ISBN",null,"3-319-02276-8"]
[null,null,"Descrizione fisica",null,"1 online resource (xiii, 148 pages) : illustrations (some color)"]
[null,null,"Collana",null,"Gale eBooks"]
[null,null,"Disciplina",null,"006.3"]
[{"$nulls":4},"620"]
[{"$nulls":4},"629.8"]
[{"$nulls":4},"629.892"]
[null,null,"Soggetti",null,"Autonomous robots"]
[{"$nulls":4},"Sailing - Technological innovations"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Part I Hardware design -- Part II Energy and power management strategies -- Part III Modeling, simulation, control, and stability analysis -- Part IV High level control architectures and algorithms."]
[null,null,null,"Sommario/riassunto","An autonomous sailboat robot is a boat that only uses the wind on its sail as propelling force, without remote control or human assistance to achieve its mission. This involves autonomy in energy (using batteries, solar panels, turbines...), sensor data processing (compass, GPS, wind sensor...), actuators control (rudder and sail angle control...) and decision making (embedded computer with adequate algorithms). Although robotic sailing is a relatively new field of research, several applications exist for this type of robots : oceanographic and hydrographic research, maritime environment monitoring, meteorology, harbor safety, assistance and rescue in dangerous areas... Over the last decade, several events such as the Microtransat challenge, the WRSC/IRSC and SailBot have been set up to stimulate research and development around robotic sailing. These proceedings cover the current and future academic and technology challenges raised by the development of autonomous sailboat robots presented at the WRSC/IRSC (World Robotic Sailing Championship/International Robotic Sailing Conference) 2013, in Brest, France, 2-6 September 2013."]