{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[18,2,18,3],[19,2,19,3],[23,2,23,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910299752003321"]
[null,null,"Autore",null,"Bolatkale Muhammed"]
[null,null,"Titolo",null,"High Speed and Wide Bandwidth Delta-Sigma ADCs / / by Muhammed Bolatkale, Lucien J. Breems, Kofi A. A. Makinwa"]
[null,null,"Pubbl/distr/stampa",null,"Cham : , : Springer International Publishing : , : Imprint : Springer, , 2014"]
[null,null,"ISBN",null,"3-319-05840-1"]
[null,null,"Edizione",null,"[1st ed. 2014.]"]
[null,null,"Descrizione fisica",null,"1 online resource (135 p.)"]
[null,null,"Collana",null,"Analog Circuits and Signal Processing, , 1872-082X"]
[null,null,"Disciplina",null,"621.39814"]
[null,null,"Soggetti",null,"Electronic circuits"]
[{"$nulls":4},"Signal processing"]
[{"$nulls":4},"Image processing"]
[{"$nulls":4},"Speech processing systems"]
[{"$nulls":4},"Electronics"]
[{"$nulls":4},"Microelectronics"]
[{"$nulls":4},"Circuits and Systems"]
[{"$nulls":4},"Signal, Image and Speech Processing"]
[{"$nulls":4},"Electronics and Microelectronics, Instrumentation"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references at the end of each chapters and index."]
[null,null,"Nota di contenuto",null,"Introduction.- Continuous-Time Delta-Sigma Modulator.- Continuous-Time Delta-Sigma Modulators at High Sampling Rates -- A 4GHz Continuous-Time ΔΣ ADC -- A 2GHz Continuous-Time ΔΣ ADC with Dynamic Error Correction.- Conclusions -- Appendices."]
[null,null,null,"Sommario/riassunto","This book describes techniques for realizing wide bandwidth (125MHz) over-sampled analog-to-digital converters (ADCs) in nanometer-CMOS processes.  The authors offer a clear and complete picture of system level challenges and practical design solutions in high-speed Delta-Sigma modulators.  Readers will be enabled to implement ADCs as continuous-time delta-sigma (CT∆Σ) modulators, offering simple resistive inputs, which do not require the use of power-hungry input buffers, as well as offering inherent anti-aliasing, which simplifies system integration. The authors focus on the design of high speed and wide-bandwidth ΔΣMs that make a step in bandwidth range which was previously only possible with Nyquist converters. More specifically, this book describes the stability, power efficiency, and linearity limits of "]
[{"$nulls":4},"ΔΣMs, aiming at a GHz sampling frequency.   • Provides overview of trends in Wide Bandwidth and High Dynamic Range analog-to-digital converters (ADCs); • Enables the design of a wide bandwidth, high dynamic range modulator with state-of-the-art power efficiency; • Includes introduction to Continuous-Time Delta-Sigma Modulators and its system level modeling; • Explains issues relating to stability of Continuous-Time Delta-Sigma Modulators; • Includes discussion of system level non-idealities in Continuous-Time Delta-Sigma Modulators; • System level design of  CT∆Σ modulators at GHz sampling frequencies; • Practical implementation details of high speed CT∆Σ ADCs; • Overview of static and dynamic error correction techniques in ∆Σ ADCs; • Dynamic error correction techniques that are suitable for high speed CT∆Σ ADCs."]