{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[23,2,23,3],[24,2,24,3],[28,2,28,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910299976503321"]
[null,null,"Autore",null,"Fridman Leonid"]
[null,null,"Titolo",null,"Robust Output LQ Optimal Control via Integral Sliding Modes / / by Leonid Fridman, Alexander Poznyak, Francisco Javier Bejarano"]
[null,null,"Pubbl/distr/stampa",null,"New York, NY : , : Springer New York : , : Imprint : Birkhäuser, , 2014"]
[null,null,"ISBN",null,"0-8176-4962-X"]
[null,null,"Edizione",null,"[1st ed. 2014.]"]
[null,null,"Descrizione fisica",null,"1 online resource (150 p.)"]
[null,null,"Collana",null,"Systems & Control: Foundations & Applications, , 2324-9749"]
[null,null,"Disciplina",null,"629.8312"]
[null,null,"Soggetti",null,"System theory"]
[{"$nulls":4},"Automatic control"]
[{"$nulls":4},"Calculus of variations"]
[{"$nulls":4},"Applied mathematics"]
[{"$nulls":4},"Engineering mathematics"]
[{"$nulls":4},"Engineering design"]
[{"$nulls":4},"Vibration"]
[{"$nulls":4},"Dynamics"]
[{"$nulls":4},"Systems Theory, Control"]
[{"$nulls":4},"Control and Systems Theory"]
[{"$nulls":4},"Calculus of Variations and Optimal Control; Optimization"]
[{"$nulls":4},"Mathematical and Computational Engineering"]
[{"$nulls":4},"Engineering Design"]
[{"$nulls":4},"Vibration, Dynamical Systems, Control"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Introduction -- Part I OPTIMAL CONTROL AND SLIDING MODE -- 2 Integral Sliding Mode Control -- 3 Observer Based on ISM -- 4 Output Integral Sliding Mode Based Control -- Part II MINI-MAX OUTPUT ROBUST LQ CONTROL -- 5 The Robust Maximum Principle -- 6 Multimodel and ISM Control -- 7 Multiplant and ISM Output Control -- 8 Fault Detection -- 9 Stewart Platform -- 10 Magnetic Bearing -- Part IV APPENDIXES -- B Min-Max Multimodel LQ Control -- Notations -- References -- Index."]
[null,null,null,"Sommario/riassunto","Featuring original research from well-known experts in the field of sliding mode control, this monograph presents new design schemes for implementing LQ control solutions in situations where the output "]
[{"$nulls":4},"system is the only information provided about the state of the plant. This new design works under the restrictions of matched disturbances without losing its desirable features. On the cutting-edge of optimal control research, Robust Output LQ Optimal Control via Integral Sliding Modes is an excellent resource for both graduate students and professionals involved in linear systems, optimal control, observation of systems with unknown inputs, and automatization. In the theory of optimal control, the linear quadratic (LQ) optimal problem plays an important role due to its physical meaning, and its solution is easily given by an algebraic Riccati equation. This solution turns out to be restrictive, however, because of two assumptions: the system must be free from disturbances and the entire state vector must be known. A new technique, called  output integral sliding modes, eliminates the effects of disturbances acting in the same subspace as the control. By using LQ-optimal control together with integral sliding modes, the former is made robust and based on output information only. Thus optimal control theory improves its applicability."]