{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[9,2,9,3],[10,2,10,3],[13,2,13,3],[13,4,13,5],[14,2,14,3],[14,4,14,5],[15,2,15,3],[15,4,15,5],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996335776703316"]
[null,null,"Titolo",null,"Advances in optical technologies"]
[null,null,"Pubbl/distr/stampa",null,"New York, NY, : Hindawi Publ"]
[null,null,"ISSN",null,"1687-6407"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Soggetti",null,"Optoelectronics"]
[{"$nulls":4},"Physics"]
[{"$nulls":4},"Optoélectronique"]
[{"$nulls":4},"Periodicals."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Periodico"]
[null,null,null,"Note generali","Refereed/Peer-reviewed"]
[null,"2.","Record Nr.",null,"UNINA9910346714803321"]
[null,null,"Autore",null,"Bejtka Ireneusz"]
[null,null,"Titolo",null,"Cross (CLT) and diagonal (DLT) laminated timber as innovative ma-terial for beam elements"]
[null,null,"Pubbl/distr/stampa",null,"KIT Scientific Publishing, 2011"]
[null,null,"ISBN",null,"1000021129"]
[null,null,"Descrizione fisica",null,"1 online resource (V, 134 p. p.)"]
[null,null,"Collana",null,"Karlsruher Berichte zum Ingenieurholzbau / Karlsruher Institut für Technologie, Lehrstuhl für Ingenieurholzbau und Baukonstruktionen"]
[null,null,"Soggetti",null,"History of engineering and technology"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Cross laminated timber (CLT) is a plate-like multi layer element with crosswise arrangement of lamellas. CLT could be used for long-span beams in particular with tensile stresses perpendicular to the beam axis. Within this work, CLT beams were optimised, resulting in diagonal orientated timber (DLT). Both CLT and DLT beams were tested in edgewise bending. Their load-carrying behaviour was studied using experimental results and finite element analysis."]