{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910346954303321"]
[null,null,"Autore",null,"Lichtenberg Klaudia"]
[null,null,"Titolo",null,"Metallmatrixverbunde mit Verstärkungselementen aus metallischem Glas Ni??Nb??Ta?? - Herstellung und Charakterisierung"]
[null,null,"Pubbl/distr/stampa",null,"KIT Scientific Publishing, 2018"]
[null,null,"ISBN",null,"1000081432"]
[null,null,"Descrizione fisica",null,"1 online resource (XVI, 402 p. p.)"]
[null,null,"Collana",null,"Schriftenreihe des Instituts für Angewandte Materialien, Karlsruher Institut für Technologie"]
[null,null,"Soggetti",null,"Technology: general issues"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","AlSi12-based metal matrix composites using metallic glass Ni??Nb??Ta?? as reinforcement were produced via gas pressure melt infiltration technique. Comprehensive investigations were performed to determine the composite´s microstructural, mechanical and thermal properties as well as damage mechanisms. The results contribute to a better understanding on the material´s processing-structure-property relations."]