{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910347053403321"]
[null,null,"Autore",null,"Weidemann Roman"]
[null,null,"Titolo",null,"Analyse der mechanischen Randbedingungen zur Adaption der oszillierenden Hinterschneidtechnik an einen Mobilbagger"]
[null,null,"Pubbl/distr/stampa",null,"KIT Scientific Publishing, 2014"]
[null,null,"ISBN",null,"1000039462"]
[null,null,"Descrizione fisica",null,"1 online resource (159 p. p.)"]
[null,null,"Collana",null,"Karlsruher Schriftenreihe Fahrzeugsystemtechnik / Institut für Fahrzeugsystemtechnik"]
[null,null,"Soggetti",null,"Technology: general issues"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The oscillating disc cutting process has shown excellent results in precisely removing area-limited-concrete structures. Due to the highly dynamic oscillatory motion, the stiffness requirements to the tool structure and the basic machine have to be considered, which is the main purpose of this work. Based on these results, a concept of a mechanical adaption of the oscillating disc cutting process to an excavator attachment tool will be developed and tested on a prototype."]