{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910389742103321"]
[null,null,"Titolo",null,"C57.13.5-2019 - IEEE Standard for Performance and Test Requirements for Instrument Transformers of a Nominal System Voltage of 115 kV and Above / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York. : , : IEEE, , 2020"]
[null,null,"ISBN",null,"1-5044-6357-9"]
[null,null,"Descrizione fisica",null,"1 online resource (81 pages)"]
[null,null,"Disciplina",null,"621.314"]
[null,null,"Soggetti",null,"Electric transformers - Standards"]
[{"$nulls":4},"Electric transformers - Testing - Standards"]
[{"$nulls":4},"High voltages"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Single-phase instrument transformers of a nominal system voltage of 115 kV and above with capacitive insulation system for line-to-ground connection and for both indoor and outdoor application are discussed in this standard. This standard is intended for use as a supplement to IEEE Std C57.13-2016 and as a basis for performance and safety of equipment. Test sequences, criteria, methods, and documentation for the test are also described."]