{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[12,2,12,3],[13,2,13,3],[17,2,17,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910437770703321"]
[null,null,"Autore",null,"Jacek Tejchman"]
[null,null,"Titolo",null,"Confined granular flow in silos : experimental and numerical investigations / / Jacek Tejchman"]
[null,null,"Pubbl/distr/stampa",null,"Cham [Germany] ; ; New York, : Springer, 2013"]
[null,null,"ISBN",null,"3-319-00318-6"]
[null,null,"Edizione",null,"[1st ed. 2013.]"]
[null,null,"Descrizione fisica",null,"1 online resource (502 p.)"]
[null,null,"Collana",null,"Springer series in geomechanics and geoengineering, , 1866-8755"]
[null,null,"Disciplina",null,"671.37"]
[null,null,"Soggetti",null,"Silos"]
[{"$nulls":4},"Bulk solids flow"]
[{"$nulls":4},"Granular materials"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Literature overview -- Analytical and standard approaches to silos -- Continuum models to bulks solids -- Model silo tests -- Large scale silo tests -- FE results within enhanced elasto-plasticity -- FE results within enhanced hypoplasticity -- Simulations of flow pattern with cellular automata."]
[null,null,null,"Sommario/riassunto","  During confined flow of bulk solids in silos some characteristic phenomena can be created, such as: —         sudden and significant increase of wall stresses, —         different flow patterns, —         formation and propagation of wall and interior shear zones, —         fluctuation of pressures and, —         strong autogenous dynamic effects. These phenomena have not been described or explained in detail yet. The main intention of the experimental and theoretical research presented in this book is to explain the above mentioned phenomena in granular bulk solids and to describe them with numerical FE models verified by experimental results."]