{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3],[12,2,12,3],[16,2,16,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910438050803321"]
[null,null,"Autore",null,"Kashmiri S. Mahdi"]
[null,null,"Titolo",null,"Electrothermal frequency references in standard CMOS / / S. Mahdi Kashmiri, Kofi A.A. Makinwa"]
[null,null,"Pubbl/distr/stampa",null,"New York, : Springer Science, 2013"]
[null,null,"ISBN",null,"1-4614-6473-0"]
[null,null,"Edizione",null,"[1st ed. 2013.]"]
[null,null,"Descrizione fisica",null,"1 online resource (ix, 214 pages) : illustrations (some color)"]
[null,null,"Collana",null,"Analog circuits and signal processing"]
[null,null,"Disciplina",null,"621.39732"]
[null,null,"Soggetti",null,"Metal oxide semiconductors"]
[{"$nulls":4},"Silicon - Electric properties"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Introduction -- Silicon-based Frequency References -- Frequency References  Based on the Thermal Properties of Silicon.-A Digitally-Assisted Electrothermal Frequency-Locked Loop in Standard CMOS -- An Electrothermal Frequency Reference in Standard 0.7µm CMOS -- A Scaled Electrothermal Frequency Reference in Standard 0.16µm CMOS -- Conclusions and Outlook -- Appendix."]
[null,null,null,"Sommario/riassunto","This book describes an alternative method of accurate on-chip frequency generation in standard CMOS IC processes. This method exploits the thermal-diffusivity of silicon, the rate at which heat diffuses through a silicon substrate.  This is the first book describing thermal-diffusivity-based frequency references, including the complete theoretical methodology supported by practical realizations that prove the feasibility of the method.  Coverage also includes several circuit and system-level solutions for the analog electronic circuit design challenges faced.   ·         Surveys the state-of-the-art in all-silicon frequency references; ·         Examines the thermal properties of silicon as a solution for the challenge of on-chip accurate frequency generation; ·         Uses simplified modeling approaches that allow an electronics engineer easily to simulate the electrothermal elements; ·         Follows a top-down methodology in circuit design, in which system-level design is promoted by behavioral simulations."]