{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3],[12,2,12,3],[13,2,13,3],[17,2,17,3],[17,4,17,5],[18,2,18,3],[18,4,18,5],[19,2,19,3],[19,4,19,5],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,2,23,3],[24,2,24,3],[25,2,25,3],[26,2,26,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910456598403321"]
[null,null,"Autore",null,"Bo Yu <1975->"]
[null,null,"Titolo",null,"High temperature electrolysis in large-scale hydrogen production [[electronic resource] /] / Yu Bo and Xu Jingming"]
[null,null,"Pubbl/distr/stampa",null,"New York, : Nova Science Publishers, Inc., c2010"]
[null,null,"ISBN",null,"1-61668-697-9"]
[null,null,"Descrizione fisica",null,"1 online resource (95 p.)"]
[null,null,"Collana",null,"Energy science, engineering and technology"]
[{"$nulls":4},"Novinka"]
[null,null,"Disciplina",null,"665.8/1"]
[null,null,"Soggetti",null,"Hydrogen as fuel"]
[{"$nulls":4},"High temperature electrolysis"]
[{"$nulls":4},"Electronic books."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,"2.","Record Nr.",null,"UNINA9910346709303321"]
[null,null,"Autore",null,"Blaß Hans JoachimSchädle, Patrick"]
[null,null,"Titolo",null,"Verhalten einer Massivholzbauweise unter Erdbebenlasten"]
[null,null,"Pubbl/distr/stampa",null,"KIT Scientific Publishing, 2011"]
[null,null,"ISBN",null,"1000023972"]
[null,null,"Descrizione fisica",null,"1 online resource (VII, 166 p. p.)"]
[null,null,"Collana",null,"Karlsruher Berichte zum Ingenieurholzbau / Karlsruher Institut für Technologie, Lehrstuhl für Ingenieurholzbau und Baukonstruktionen"]
[null,null,"Soggetti",null,"History of engineering and technology"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Die Eigenschaften einer Massivholzbauweise, die aufgrund ihrer Flexibilität und des einfachen Aufbaus besonders für den Einsatz in Erdbebengebieten geeignet ist, wurden untersucht. In experimentellen Untersuchungen wurden die Eigenschaften der Verbindungsmittel und von Wandscheiben in Originalgröße geprüft. Mit Hilfe numerischer Modelle wurde das Verhalten der Bauweise unter monotonen und zyklischen Lasten berechnet. Mit den Modellen wurde der Verhaltensbeiwert q bestimmt."]