{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[12,2,12,3],[13,2,13,3],[17,2,17,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910465404303321"]
[null,null,"Autore",null,"Iu Herbert Ho-Ching"]
[null,null,"Titolo",null,"Development of memristor based circuits [[electronic resource] /] / Herbert Ho-Ching Iu, Andrew L. Fitch"]
[null,null,"Pubbl/distr/stampa",null,"New Jersey ; ; London, : World Scientific, c2013"]
[null,null,"ISBN",null,"1-299-28119-2"]
[{"$nulls":4},"981-4383-39-2"]
[null,null,"Descrizione fisica",null,"1 online resource (133 p.)"]
[null,null,"Collana",null,"World Scientific series on nonlinear science, Series A, , 1793-1010 ; ; v. 82"]
[null,null,"Disciplina",null,"621.3815"]
[null,null,"Soggetti",null,"Memristors"]
[{"$nulls":4},"Electronic circuits"]
[{"$nulls":4},"Electronic books."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Contents; Preface; 1 Introduction; 1.1 Introduction; 1.2 HP Memristor; 1.3 Memristor Emulator; 1.3.1 Valsa's memristor emulator; 1.3.2 Pershin and Di Ventra's memristor emulator; 1.3.3 Muthuswamy's memristor modeling circuit; 1.3.4 Kim's memristor emulating circuit; 1.4 Structure of the Book; References; 2 Controlling Chaos in a Memristor Based Circuit; 2.1 Introduction; 2.2 Memristor Based Chaotic Circuit; 2.3 Notch Filter Feedback Controller; 2.3.1 Twin-T notch filter; 2.3.2 Interface circuit; 2.4 Simulation Results; 2.5 Experimental Setup; 2.6 Conclusion; References"]
[{"$nulls":4},"3 Hyperchaos in a Memristor Based Modified Canonical Chua's Circuit3.1 Introduction; 3.2 Dynamical Equations of MHC; 3.3 Simulation Results; 3.4 Experimental Setup; 3.5 Conclusion; References; 4 Realization of an Analog Model of a Memristor Based on a Light Dependent Resistor; 4.1 Introduction; 4.2 Circuit Objectives; 4.3 Simulation Setup; 4.4 Experimental Setup; 4.5 Conclusion; References; 5 Design of a Memcapacitor Emulator Based on a Memristor; 5.1 Introduction; 5.2 The Memcapacitor and Its Relation to the Memristor; 5.3 Simulation Setup; 5.4 Experimental Setup; 5.5 Conclusion; References"]
[{"$nulls":4},"6 Practical Realization of an Analog Model of a Memcapacitor6.1 Introduction; 6.2 Circuit Description; 6.2.1 Memristor mimicking circuit; 6.2.2 Capacitor multiplier; 6.2.3 Memcapacitor emulator; 6.3 Experimental Setup; 6.4 Conclusion; References; 7 Chaos in "]
[{"$nulls":4},"Memristively Coupled Harmonic Oscillators; 7.1 Introduction; 7.2 Coupled Oscillator Circuits; 7.3 Memristor Mimicking Circuit; 7.4 Memristively Coupled Harmonic Oscillator Circuit; 7.5 Experimental Setup; 7.6 Conclusion; References; 8 Conclusion and Future Work; 8.1 Summary; 8.2 Memory Applications; 8.3 Low Power Devices and Sensing"]
[{"$nulls":4},"8.4 Neuromorphic Applications8.5 Flexible Circuits; 8.6 Analog Applications; References; Index"]
[null,null,null,"Sommario/riassunto","In 1971, Leon O. Chua presented the formulation of a memristor, which was postulated as the fourth circuit element in electrical circuit theory - one that could join the existing core group of elements: capacitor, resistor and inductor. For over thirty years, the memristor had held no significance in circuit theory. Then in 2008, a group of scientists from Hewlett-Packard Labs (HP) developed a working memristor. Although the solid state implementation of the memristor inspired appreciable interest in developing applications, memristors are not yet available on the market to date. HP labs do no"]