{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910488732803321"]
[null,null,"Titolo",null,"1904.2-2021 - IEEE standard for control and management of virtual links in ethernet-based subscriber access networks / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 2021"]
[null,null,"ISBN",null,"1-5044-7710-3"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"004.68"]
[null,null,"Soggetti",null,"Ethernet (Local area network system)"]
[{"$nulls":4},"Network performance (Telecommunication)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Control mechanisms and management methods necessary to enable creation and operation of virtual links in Ethernet-based subscriber access networks are described. The key characteristics of the Virtual Link Control (VLC) mechanisms are: - The ability to transit Layer 2 bridges in a single IEEE 802 Media Access Control (MAC) domain to allow remote device management - Extensibility to accommodate new protocols and new types of devices - The ability to simultaneously send messages to multiple VLC-aware stations using broadcast or multicast addressing The message format, as well as processing operations at the stations participating in the VLC protocol, are described."]