{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910502639603321"]
[null,null,"Autore",null,"Pronk Arno"]
[null,null,"Titolo",null,"Flexible forming for fluid architecture / / Arno Pronk"]
[null,null,"Pubbl/distr/stampa",null,"Cham, Switzerland : , : Springer, , [2021]"]
[{"$nulls":4},"©2021"]
[null,null,"ISBN",null,"3-030-71551-5"]
[null,null,"Descrizione fisica",null,"1 online resource (586 pages)"]
[null,null,"Disciplina",null,"624.17762"]
[null,null,"Soggetti",null,"Shells (Engineering)"]
[{"$nulls":4},"Structural engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This book on flexible formwork for fluid architecture is a multi-faceted research that covers a broad field: from design to material and technology, and from history to future developments. It offers a pragmatic approach that can be extended with more cases, materials, techniques and methods for fluid architecture, and provides a better understanding of the main aspects of fluid architecture and to help them find the most suitable combinations of all aspects.The book is a challenging experience with many new discoveries, including two patents: one on moulding of fluid surfaces and one on 3D printing of fibre-reinforced ice. It also features two world records: the larges span (30 meters) and the highest thin shell structure (30,5 meters) in ice as well as a method for the construction of a fully laminated shell structure in insulated glass."]