{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910557117503321"]
[null,null,"Titolo",null,"Intermetallic Compound"]
[null,null,"Pubbl/distr/stampa",null,"Basel, Switzerland, : MDPI - Multidisciplinary Digital Publishing Institute, 2021"]
[{"$nulls":4},"Basel, Switzerland : , : MDPI - Multidisciplinary Digital Publishing Institute, , 2021"]
[null,null,"Descrizione fisica",null,"1 online resource (138 p.)"]
[null,null,"Soggetti",null,"History of engineering and technology"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This Special Issue collects ten articles related to the broadly understood physical properties of intermetallic compounds. Differential thermal analysis was carried out, and the temperatures of thermal effects that arise during the reduction of neodymium from a technological salt mixture of KCl-NaCl-CaCl2-NdF3 with a magnesium-zinc alloy were established. For sol-gel products of stoichiometric MgTiO3, accurate thermal expansion coefficients were measured. The effect of various nanoparticles, such as GaF3, ZnF2, Zn(BF4)2 and Ga2O3 additions, on the activity of CsF-RbF-AlF3 flux and mechanical behavior of Al/Steel brazed joints is presented. The effect of Bi substitution on the structural and magnetic properties of Nd1-xBixMnO3 is investigated. Characteristics of hard magnetic materials based on Nd2Fe14B and Ce2Fe14B intermetallic compounds are presented. A special algorithm is presented to support vector regression for estimating the maximum magnetic entropy change of doped manganite-based compounds. We have received information about the mechanical properties of the reactively synthesized porous Ti3SiC2 compound with different apertures. Furthermore, we have presented the experimental results of Zn-doped Al-rich for fast on-board hydrogen production."]