{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[7,2,7,3],[8,2,8,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910566467403321"]
[null,null,"Author",null,"Chen Su-Chin"]
[null,null,"Title",null,"Soil-Water Conservation, Erosion, and Landslide"]
[null,null,"Publication",null,"Basel, : MDPI - Multidisciplinary Digital Publishing Institute, 2022"]
[null,null,"Physical description",null,"1 online resource (392 p.)"]
[null,null,"Subjects",null,"Environmental science, engineering and technology"]
[{"$nulls":4},"Technology: general issues"]
[null,null,"Language",null,"English"]
[null,null,"Format",null,"Language material"]
[null,null,null,"Bibliographic level","Monograph"]
[null,null,null,"Summary, etc","The predicted climate change is likely to cause extreme storm events and, subsequently, catastrophic disasters, including soil erosion, debris and landslide formation, loss of life, etc. In the decade from 1976, natural disasters affected less than a billion lives. These numbers have surged in the last decade alone. It is said that natural disasters have affected over 3 billion lives, killed on average 750,000 people, and cost more than 600 billion US dollars. Of these numbers, a greater proportion are due to sediment-related disasters, and these numbers are an indication of the amount of work still to be done in the field of soil erosion, conservation, and landslides. Scientists, engineers, and planners are all under immense pressure to develop and improve existing scientific tools to model erosion and landslides and, in the process, better conserve the soil. Therefore, the purpose of this Special Issue is to improve our knowledge on the processes and mechanics of soil erosion and landslides. In turn, these will be crucial in developing the right tools and models for soil and water conservation, disaster mitigation, and early warning systems."]
[null,"2.","Record Nr.",null,"UNINA9910346778203321"]
[null,null,"Author",null,"Plum Robin Marc"]
[null,null,"Title",null,"Fatigue crack detection on structural steel members by using ultrasound excited thermography = Erkennung von Ermüdungsrissen in Stahlbauteilen durch ultraschallangeregte Thermografie"]
[null,null,"Publication",null,"KIT Scientific Publishing, 2015"]
[null,null,"ISBN",null,"1000048191"]
[null,null,"Physical description",null,"1 online resource (XVI, 334 p. p.)"]
[null,null,"Series statement",null,"Berichte zum Stahl- und Leichtbau / Karlsruher Institut für Technologie, Versuchsanstalt für Stahl, Holz und Steine, Stahl- und Leichtbau"]
[null,null,"Subjects",null,"Technology: general issues"]
[null,null,"Language",null,"English"]
[null,null,"Format",null,"Language material"]
[null,null,null,"Bibliographic level","Monograph"]
[null,null,null,"Summary, etc","Ultrasound excitation of structural steel members leads to localised energy dissipation at existent fatigue cracks and thus allows for thermographic flaw detection. Essential effects on the defect-selective heating, such as flaw size, plate thickness, crack mouth opening or static preload, are systematically investigated. Laser vibrometry measurements of the crack edges, theoretical modelling of frictional heating and numerical simulations contribute to the understanding of the involved physics."]