{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910566489603321"]
[null,null,"Autore",null,"Binninger Marco"]
[null,null,"Titolo",null,"Untersuchungen zum Arbeitsfluss in getakteten Bauproduktionssystemen aus Perspektive von Generalunternehmern / / Marco Binninger"]
[null,null,"Pubbl/distr/stampa",null,"Karlsruhe : , : KIT Scientific Publishing, , 2022"]
[null,null,"Descrizione fisica",null,"1 online resource (xxiv, 244 Seiten) : illustrations"]
[null,null,"Disciplina",null,"658.5"]
[null,null,"Soggetti",null,"Production management"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Ein guter Arbeitsfluss spielt in der Produktion eine maßgebende Rolle hinsichtlich der Produktivität und Effizienz. Im Bauwesen sorgt der Einsatz des Taktes für die Erzeugung des Flusses. Die vorliegende Arbeit nimmt sich dem Fluss und dem Takt im Bauwesen an. Es wird eine Arbeitsflussbewertungsmatrix für getaktete Bauprojekte hergeleitet und 50 Bauprojekte damit untersucht. Es kann ein theoretisches Verbesserungspotential von bis zu 80% hinsichtlich der Arbeitsflusseffizienz aufgezeigt werden. - A good workflow plays a crucial role in production in terms of productivity and efficiency. In construction, the use of tact creates flow. The scientific work takes on the flow and tact in construction. A workflow evaluation matrix for tacted construction projects is derived and 50 construction projects are examined with it. A theoretical potential for improvement of up to 80% in terms of workflow efficiency can be demonstrated. With the help of the derived improvement approaches including more."]