{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[12,2,12,3],[13,2,13,3],[16,2,16,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910568248003321"]
[null,null,"Autore",null,"Zhang Wenrui"]
[null,null,"Titolo",null,"Oxide-ion conduction in the Dion-Jacobson-type layered perovskites / / Wenrui Zhang"]
[null,null,"Pubbl/distr/stampa",null,"Singapore : , : Springer, , [2022]"]
[{"$nulls":4},"©2022"]
[null,null,"ISBN",null,"9789811922473"]
[{"$nulls":4},"9789811922466"]
[null,null,"Descrizione fisica",null,"1 online resource (135 pages)  ; : illustrations (chiefly color)"]
[null,null,"Collana",null,"Springer Theses."]
[null,null,"Disciplina",null,"537.622"]
[null,null,"Soggetti",null,"Electric conductivity"]
[{"$nulls":4},"Electric conductivity - Measurement"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","\"Doctoral thesis accepted by Tokyo Institute of Technology, Tokyo, Japan.\""]
[null,null,"Nota di contenuto",null,"1. Introduction --2. New Oxide-ion conductors of DionJacobson-Type Layered Perovskites CsBi₂Ti₂NbO₁₀[delta] --3. New Oxide-ion conductors of DionJacobson- Type Layered Perovskites CsLn₂Ti2₂NbO₁₀ (Ln = La, Pr, Nd, Sm, Gd, Ho and Yb) and CsLa₂xMxTi₂+yNb₁yO₁₀x/₂y/₂ (M = Ca, Sr and Ba; x = 0, 0.1; y = 0.1, 0 and 0.1) --4. Conclusion and Future Work. ."]
[null,null,null,"Sommario/riassunto","This book reports a study of a class of DionJacobson-type layered perovskite oxides in which high oxide-ion conductivities in phases were discovered for the first time in the world. The oxide-ion conductors are important in various energy conversion devices and environmental protection applications such as solid-oxide fuel cells, oxygen gas sensors, oxygen separation membranes, and oxygen-based catalysts."]