{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910633982003321"]
[null,null,"Autore",null,"Stantchev Rayko Ivanov"]
[null,null,"Titolo",null,"Spatial Terahertz-Light Modulators for Single-Pixel Cameras / / written by Rayko Ivanov Stantchev and Emma Pickwell-MacPherson"]
[null,null,"Pubbl/distr/stampa",null,"London : , : IntechOpen, , 2021"]
[null,null,"ISBN",null,"1-83962-684-4"]
[null,null,"Descrizione fisica",null,"1 online resource (202 pages)"]
[null,null,"Disciplina",null,"543.5"]
[null,null,"Soggetti",null,"Terahertz spectroscopy"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,"Nota di contenuto",null,"1. Introduction -- 2. Single-pixel imaging theory -- 3. Spatially modulating THz radiation -- 3.1 Mechanical masks -- 3.2 THz modulation by charge carrier injection/depletion -- 3.2.1 Optical modulators -- 3.2.2 Electrical modulators -- 3.3 Spatially patterned THz generation -- 3.4 Liquid crystal THz modulators -- 4. Applications and discussion -- 5. Conclusions -- Acknowledgments -- Conflict of interest -- Nomenclature -- References."]
[null,null,null,"Sommario/riassunto","Terahertz imaging looks set to become an integral part of future applications from semiconductor quality control to medical diagnosis. This will only become a reality when the technology is sufficiently cheap and capabilities adequate to compete with others. Single-pixel cameras use a spatial light modulator and a detector with no spatial-resolution in their imaging process. The spatial-modulator is key as it imparts a series of encoding masks on the beam and the detector measures the dot product of each mask and the object, thereby allowing computers to recover an image via post-processing. They are inherently slower than parallel-pixel imaging arrays although they are more robust and cheaper, hence are highly applicable to the terahertz regime. This chapter dedicates itself to terahertz single-pixel cameras; their current implementations, future directions and how they compare to other terahertz imaging techniques. We start by outlining the competing imaging techniques, then we discuss the theory behind single-pixel imaging; the main section shows the methods of spatially modulating a terahertz beam; and finally there is a discussion about the future limits of such cameras and the concluding remarks express the authors' vision for the future of single-pixel THz cameras."]