{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910647223903321"]
[null,null,"Titolo",null,"Polymers and Their Application in 3D Printing / / Hamid Reza Vanaei, Sofiane Khelladi, Abbas Tcharkhtchi, editors"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : MDPI - Multidisciplinary Digital Publishing Institute, , 2023"]
[null,null,"ISBN",null,"3-0365-6028-9"]
[null,null,"Descrizione fisica",null,"1 online resource (182 pages)"]
[null,null,"Disciplina",null,"620.192"]
[null,null,"Soggetti",null,"Polymers - Rheology"]
[{"$nulls":4},"Polymers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,"Nota di contenuto",null,"Effects of Laser Power and Hatch Orientation on Final Properties of PA12 Parts Produced by Selective Laser Sintering 1 -- Strain Release Behaviour during Crack Growth of a Polymeric Beam under Elastic Loads for Self-Healing 23 -- Piezoresistive Properties of 3D-Printed Polylactic Acid (PLA) Nanocomposites 51 -- Characterization of 3D Printed Metal-PLA Composite Scaffolds for Biomedical Applications 63 -- Modeling Impact Mechanics of 3D Helicoidally Architected Polymer Composites Enabled by Additive Manufacturing for Lightweight Silicon Photovoltaics Technology 75 -- Clinical Application of 3D-Printed Patient-Specific Polycaprolactone/Beta Tricalcium Phosphate Scaffold for Complex Zygomatico-Maxillary Defects 93 -- Effect of Architected Structural Members on the Viscoelastic Response of 3D Printed Simple Cubic Lattice Structures 107 -- Effect of Printing Process Parameters on the Shape Transformation Capability of 3D Printed Structures 123 -- 3D Bioprinting of Polycaprolactone-Based Scaffolds for Pulp-Dentin Regeneration: Investigation of Physicochemical and Biological Behavior 145 -- 3D Printed and Conventional Membranes-A Review 159."]
[null,null,null,"Sommario/riassunto","Fused filament fabrication, also known as 3D printing, is extensively used to produce prototypes for applications in, e.g., the aerospace, medical, and automotive industries. In this process, a thermoplastic polymer is fed into a liquefier that extrudes a filament while moving in successive X-Y planes along the Z direction to fabricate a 3D part in a layer-by-layer process. Due to the progressive advances of this process in industry, the application of polymeric (or even composite) materials have received much attention. Researchers and industries now engage "]
[{"$nulls":4},"in 3D printing by implementing numerous polymeric materials in their domain. In this Special Issue, we will present a collection of recent and novel works regarding the application of polymers in 3D printing."]