{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[15,2,15,3],[16,2,16,3],[19,2,19,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910659492503321"]
[null,null,"Autore",null,"Zhu Zhehao"]
[null,null,"Titolo",null,"Influence of Fine Particles on the Liquefaction Properties of a Reference Sand : Application to the Seismic Response of a Sand Column on a Vibrating Table / / by Zhehao Zhu"]
[null,null,"Pubbl/distr/stampa",null,"Cham : , : Springer Nature Switzerland : , : Imprint : Springer, , 2023"]
[null,null,"ISBN",null,"9783031242991"]
[{"$nulls":4},"9783031242984"]
[null,null,"Edizione",null,"[1st ed. 2023.]"]
[null,null,"Descrizione fisica",null,"1 online resource (208 pages)"]
[null,null,"Collana",null,"Springer Theses, Recognizing Outstanding Ph.D. Research, , 2190-5061"]
[null,null,"Disciplina",null,"551.22"]
[null,null,"Soggetti",null,"Engineering geology"]
[{"$nulls":4},"Geotechnical engineering"]
[{"$nulls":4},"Geophysics"]
[{"$nulls":4},"Geoengineering"]
[{"$nulls":4},"Geotechnical Engineering and Applied Earth Sciences"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Bibliographic Review -- Tested Materials, Equipment and Protocols -- Behaviour Under Monotonic Loading -- Behaviour Under Cyclic Loading -- Shaking Table Tests."]
[null,null,null,"Sommario/riassunto","Over the past thirty years, the liquefaction of sand containing a small amount of fine particles has become an engaging topic in the geotechnical community. Indeed, a great variety of field investigations revealed that the real liquefied soils are mainly composed of a host sand matrix and a small fraction of plastic or non-plastic fines. In this context, several series of monotonic and cyclic triaxial tests were performed to clarify the influence of these fine particles on the development of sand liquefaction. To get closer to in situ conditions, 1g shaking table tests were carried out with two different-sized model soil containers. The first one, small size, was essentially used to check the reconstitution and the saturation method. The second one, very large size, was manufactured to explore the sand liquefaction behaviour during base shaking in an almost actual engineering size. To numerically reproduce the sand liquefaction behaviour, the Dafalias model has been taken as an exampleand its input parameters were calibrated by an artificial intelligence method. An in-depth analysis of "]
[{"$nulls":4},"the proposed method was done with the elastoplastic theory."]