{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3],[12,2,12,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910693810303321"]
[null,null,"Autore",null,"Hausner Michael"]
[null,null,"Titolo",null,"Specifications and Standards for Optical Coating Durability"]
[null,null,"Pubbl/distr/stampa",null,"Bellingham : , : Society of Photo-Optical Instrumentation Engineers, , 2019"]
[{"$nulls":4},"©2019"]
[null,null,"ISBN",null,"1-5106-3048-1"]
[null,null,"Descrizione fisica",null,"1 online resource (49 pages)"]
[null,null,"Collana",null,"SPIE. Spotlight ; ; SL51"]
[null,null,"Disciplina",null,"621.36"]
[null,null,"Soggetti",null,"Optical coatings"]
[{"$nulls":4},"Optical coatings - Testing"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Preface -- 1. Purpose -- 2. Glossary -- 3. Environmental durability of optical coatings: 3.1. Common durability requirements for optical coatings; 3.2. Laser damage threshold durability for optical coating; 3.3. Windscreen wiper test; 3.4. Rain erosion test; 3.5. Optical coating durability in industrial oils and fuels; 3.6. Durability testing of coating on actual component - when? 3.7. Visual inspection/examination -- 4. Characterization of optical coatings: 4.1. Functionality of the coating; 4.2. Spectral region of the coating -- 5. Factors impacting the quality of the coating: 5.1. Coating materials' composition; 5.2. Raw material of the element's substrate; 5.3. Optical performance; 5.4. Environmental durability for which the coated element should be resistant; 5.5. Size and shape of the element; 5.6. Cleaning of the optical surfaces; 5.7. Additional factors -- 6. Environmental durability: equipment, tools, and materials for testing: 6.1. Equipment and tools; 6.2. Materials -- 7. Quality and safety aspects: 7.1. Quality aspects; 7.2. Safety aspects -- 8. Environmental durability requirements and test conditions according to accepted standards and specifications: 8.1. MIL-M-13508C (1973); 8.2. MIL-F-48616 (1977); 8.3. MIL-C-48497A (1980); 8.4. MIL-C-14806A (1969); 8.5. MIL-C-675C (1980); 8.6. MIL-PRF-13830B (1997); 8.7. MIL-STD-810G (2008); 8.8. ISO 9211-3 (2010); 8.9. TS-1888 (1979) -- 9. Examples of failed coatings on witness samples or elements during environmental durability test -- 10. Summary -- Appendix: List of publications -- Acknowledgments."]
[null,null,null,"Sommario/riassunto","This Spotlight gives a general overview of the durability of optical "]
[{"$nulls":4},"coatings and various durability tests referring to available civilian and military standards and specifications. It will allow a quick detection of the coating testing durability requirements and test conditions in MIL-Specs and other standards or specifications according to requirements defined in the relevant drawings or coating specifications. Intended for optical designers, this Spotlight is also useful for optical coating inspectors."]