{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[22,2,22,3],[23,2,23,3],[27,2,27,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279565503316"]
[null,null,"Titolo",null,"ANSI/IEEE Std 936-1987 : IEEE Guide for Self-Commutated Converters / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, NJ : , : IEEE, , 1987"]
[null,null,"ISBN",null,"0-7381-4265-4"]
[null,null,"Descrizione fisica",null,"1 online resource (40 pages)"]
[null,null,"Disciplina",null,"621.3815322"]
[null,null,"Soggetti",null,"Electric current converters"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This guide applies to self-commutated electronic power converters in which commutation is accomplished by components within the converter. In converters using switching devices that have turn-off capability, such as transistors or gate turn-off thyristors, interruption of the current results in a voltage that commutates the current to another branch. In converters using circuit-commutated thyristors, the commutating voltages required to transfer current from one branch to another are normally supplied by capacitors. The type of power conversion may be DC to AC, DC to DC, AC to DC, or AC to AC. Converters in which commutating voltages are supplied by the AC lines, the AC load, or some other AC source outside the converter, are excluded from the scope of this guide except where they may be linked with a self-commutated converter."]
[null,"2.","Record Nr.",null,"UNINA9910790136703321"]
[null,null,"Titolo",null,"Nuclear corrosion science and engineering [[electronic resource] /] / edited by Damien Feron"]
[null,null,"Pubbl/distr/stampa",null,"Cambridge, : Woodhead Pub., 2012"]
[null,null,"ISBN",null,"0-85709-534-X"]
[null,null,"Descrizione fisica",null,"1 online resource (1073 p.)"]
[null,null,"Collana",null,"Woodhead publishing series in energy, , 2044-9364 ; ; no. 22"]
[null,null,"Disciplina",null,"621.483"]
[null,null,"Soggetti",null,"Nuclear reactors - Corrosion"]
[{"$nulls":4},"Corrosion and anti-corrosives"]
[{"$nulls":4},"Nuclear power plants"]
[{"$nulls":4},"Nuclear engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"pt. 1. Introduction to corrosion in nuclear power applications -- pt. 2. Aqueous corrosion in nuclear power applications : fundamental science, materials and mechanisms -- pt. 3. Non-aqueous corrosion in nuclear power applications : fundamental science, materials and mechanisms -- pt. 4. Corrosion monitoring and control in nuclear power applications -- pt. 5. Corrosion issues in current nuclear reactors and applications -- pt. 6. Corrosion issues in next generation nuclear reactors and advanced applications."]
[null,null,null,"Sommario/riassunto","Corrosion of nuclear materials, i.e. the interaction between these materials and their environments, is a major issue for plant safety as well as for operation and economic competitiveness. Understanding these corrosion mechanisms, the systems and materials they affect, and the methods to accurately measure their incidence is of critical importance to the nuclear industry. Combining assessment techniques and analytical models into this understanding allows operators to predict the service life of corrosion-affected nuclear plant materials, and to apply the most appropriate maintenance and miti"]