{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910795477703321"]
[null,null,"Autore",null,"Classen Christoph"]
[null,null,"Titolo",null,"Effiziente Simulation elektromagnetischer Felder durch Kantenkorrektur und spektralbasierte Interpolation / / vorgelegt von Christoph Classen"]
[null,null,"Pubbl/distr/stampa",null,"Berlin : , : Logos Verlag Berlin GmbH, , [2015]"]
[{"$nulls":4},"©2015"]
[null,null,"ISBN",null,"3-8325-9525-2"]
[null,null,"Descrizione fisica",null,"1 online resource (x, 157 pages) : illustrations"]
[null,null,"Disciplina",null,"003.3"]
[null,null,"Soggetti",null,"Computer simulation"]
[{"$nulls":4},"Electromagnetic fields"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","PublicationDate: 20150220"]
[null,null,null,"Sommario/riassunto","Long description: Bei der Simulation elektromagnetischer Felder kommt es häufig zu Problemstellungen, die mit den üblichen numerischen Verfahren nicht effizient gelöst werden können.  Dieses Buch befasst sich mit singulären Feldverläufen an Materialkanten sowie der Berechnung hochresonanter Strukturen.  Es werden Lösungen erarbeitet, die die Rechenzeit der Simulation deutlich reduzieren und gleichzeitig die Genauigkeit der Lösung erhöhen können. Hierbei werden die Formulierungen der Methode der finiten Integration (FIT) genutzt, um die Zusammenhänge und Erweiterungen anschaulich darzustellen. Alle Erweiterungen erfolgen im Pre- oder Postprocessing und sind so gut in bestehende Programme zu integrieren und leicht auf andere numerische Verfahren (z.B. finite Differenzen) übertragbar."]