{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910806928603321"]
[null,null,"Autore",null,"El-Gendy Nour Shafĭk"]
[null,null,"Titolo",null,"Biodesulfurization in petroleum refining / / Nour Shafik El-Gendy, Hussein Mohamed Nabil Nassar"]
[null,null,"Pubbl/distr/stampa",null,"Hoboken, New Jersey ; ; Beverly, Massachusetts : , : Scrivener Publishing : , : Wiley, , 2018"]
[null,null,"ISBN",null,"1-119-22410-1"]
[{"$nulls":4},"1-119-22408-X"]
[{"$nulls":4},"1-119-22407-1"]
[null,null,"Edizione",null,"[1st edition]"]
[null,null,"Descrizione fisica",null,"1 online resource (1,198 pages)"]
[null,null,"Disciplina",null,"665.53"]
[null,null,"Soggetti",null,"Petroleum - Refining - Desulfurization"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,null,"Sommario/riassunto","Petroleum refining and process engineering is constantly changing.  No new refineries are being built, but companies all over the world are still expanding or re-purposing huge percentages of their refineries every year, year after year.  Rather than building entirely new plants, companies are spending billions of dollars in the research and development of new processes that can save time and money by being more efficient and environmentally safer. Biodesulfurization is one of those processes, and nowhere else it is covered more thoroughly or with more up-to-date research of the new advances than in this new volume from Wiley-Scrivener.  Crude oil consists of hydrocarbons, along with other minerals and trace elements.  Sulfur is the most abundant element after carbon and hydrogen, then comes after it nitrogen, and they usually concentrated in the higher boiling fractions of the crude oil. The presence of sulfur compounds causes the corrosion of refining facilities and catalysts poisoning. Moreover, the presence of nitrogen-compounds directly impacts the refining processes via; poisoning the cracking catalysts and inhibiting the hydrodesulfurization catalysts. In addition, both have bad impacts on the environment, throughout the sulfur and nitrogen oxide emissions. Removing this sulfur and nitrogen from the refining process protects equipment and the environment and creates a more efficient and cost-effective process.  Besides the obvious benefits to biodesulfurization, "]
[{"$nulls":4},"there are new regulations in place within the industry with which companies will, over the next decade or longer, spend literally tens, if not hundreds, of billions of dollars to comply.  Whether for the veteran engineer needing to update his or her library, the beginning engineer just learning about biodesulfurization, or even the student in a chemical engineering class, this outstanding new volume is a must-have. Especially it covers also the bioupgrading of crude oil and its fractions, biodenitrogenation technology and application of nanotechnology on both bio-desulfurization and denitrogenation technologies."]