{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910829958103321"]
[null,null,"Autore",null,"Kazimierczuk Marian K."]
[null,null,"Titolo",null,"Average current-mode control of DC-DC power converters / / Marian K. Kazimierczuk, Dalvir K. Saini, Agasthya Ayachit"]
[null,null,"Pubbl/distr/stampa",null,"Hoboken, New Jersey : , : John Wiley & Sons, Inc., , [2022]"]
[{"$nulls":4},"©2022"]
[null,null,"ISBN",null,"1-119-52568-3"]
[{"$nulls":4},"1-119-52559-4"]
[{"$nulls":4},"1-119-52556-X"]
[null,null,"Descrizione fisica",null,"1 online resource (339 pages)"]
[null,null,"Disciplina",null,"621.3132"]
[null,null,"Soggetti",null,"Electric controllers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Includes index."]
[null,null,null,"Sommario/riassunto","\"The book is aimed at the development of small-signal models and transfer functions related to the inner current and outer voltage loops. Then, the inner loop with average current-mode control is analysed and the dynamic characteristic will be determined for the benefit of power supply designers. First a solid understanding will be established for average current-mode control of basic power converter topologies such as buck, boost, and buck-boost converters in continuous-conduction mode (CCM). Subsequently, more advanced converters such as fly back, impedance-source, and dual-SEPIC (or zeta) converters will be considered.\"--"]