{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910915688003321"]
[null,null,"Autore",null,"IAEA"]
[null,null,"Titolo",null,"Assessment of Aircraft Accident Conditions in the Context of Test Requirements for Type C Packages Containing Radioactive Material"]
[null,null,"Pubbl/distr/stampa",null,"Vienna : , : International Atomic Energy Agency, , 2021"]
[{"$nulls":4},"©2021"]
[null,null,"ISBN",null,"92-0-121621-1"]
[null,null,"Edizione",null,"[1st ed.]"]
[null,null,"Descrizione fisica",null,"1 online resource (147 pages)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The IAEA Regulations for the safe transport of radioactive material specify test requirements for Type C packages, which are used for shipments of radioactive material by air. From 1998 to 2006, the IAEA conducted a coordinated research project (CRP) to assess aircraft accident frequency and severity in the context of Type C package test requirements. This publication presents the outcome of the original research conducted under the CRP. The results are expected to lead to increased knowledge of the post-crash survivability of packages containing high activity radioactive material."]