{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[17,2,17,3],[18,2,18,3],[22,2,22,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910953937503321"]
[null,null,"Autore",null,"Isermann Rolf"]
[null,null,"Titolo",null,"Digital Control Systems : Volume 2: Stochastic Control, Multivariable Control, Adaptive Control, Applications / / by Rolf Isermann"]
[null,null,"Pubbl/distr/stampa",null,"Berlin, Heidelberg : , : Springer Berlin Heidelberg : , : Imprint : Springer, , 1991"]
[null,null,"ISBN",null,"3-642-86420-1"]
[null,null,"Edizione",null,"[2nd ed. 1991.]"]
[null,null,"Descrizione fisica",null,"1 online resource (XXI, 325 p.)"]
[null,null,"Disciplina",null,"629.8"]
[null,null,"Soggetti",null,"Automatic control"]
[{"$nulls":4},"Robotics"]
[{"$nulls":4},"Automation"]
[{"$nulls":4},"Engineering mathematics"]
[{"$nulls":4},"Engineering - Data processing"]
[{"$nulls":4},"Computers"]
[{"$nulls":4},"Control, Robotics, Automation"]
[{"$nulls":4},"Mathematical and Computational Engineering Applications"]
[{"$nulls":4},"Computer Hardware"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"C Control Systems for Stochastic Disturbances -- 12 Stochastic Control Systems (Introduction) -- 13 Parameter-optimized Controllers for Stochastic Disturbances -- 14 Minimum Variance Controllers for Stochastic Disturbances -- 15 State Controllers for Stochastic Disturbances -- D Interconnected Control Systems -- 16 Cascade Control Systems -- 17 Feedforward Control -- E Multivariable Control Systems -- 18 Structures of Multivariable Processes -- 19 Parameter-optimized Multivariable Control Systems -- 20 Multivariable Matrix Polynomial Control Systems -- 21 Multivariable State Control Systems -- 22 State Estimation -- F Adaptive Control Systems -- 23 Adaptive Control Systems (A Short Review) -- 24 On-line Identification of Dynamical Processes and Stochastic Signals -- 25 On-line Identification in Closed Loop -- 26 Parameter-adaptive Controllers -- G Digital Control with Process Computers and Microcomputers -- 27 The Influence of Amplitude Quantization for Digital Control -- 28 Filtering of Disturbances -- 29 Combining Control Algorithms and Actuators -- 30 Computer-aided Control Algorithm Design -- 31 Adaptive and "]
[{"$nulls":4},"Selftuning Control Systems Using Microcomputers and Process Computers -- References."]
[null,null,null,"Sommario/riassunto","The great advances made in large-scale integration of semiconductors and the resulting cost-effective digital processors and data storage devices determine the present development of automation. The application of digital techniques to process automation started in about 1960, when the first process computer was installed. From about 1970 process computers with cathodic ray tube display have become standard equipment for larger automation systems. Until about 1980 the annual increase of process computers was about 20 to 30%. The cost of hardware has already then shown a tendency to decrease, whereas the relative cost of user software has tended to increase. Because of the high total cost the first phase of digital process automation is characterized by the centralization of many functions in a single (though sometimes in several) process computer. Application was mainly restricted to medium and large processes. Because of the far-reaching consequences of a breakdown in the central computer parallel standby computers or parallel back-up systems had to be provided. This meant a substantial increase in cost. The tendency to overload the capacity and software problems caused further difficulties. In 1971 the first microprocessors were marketed which, together with large-scale integrated semiconductor memory units and input/output modules, can be assem­ bled into cost-effective microcomputers. These microcomputers differ from process computers in fewer but higher integrated modules and in the adaptability of their hardware and software to specialized, less comprehensive tasks."]