{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[13,2,13,3],[14,2,14,3],[18,2,18,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9911004814903321"]
[null,null,"Titolo",null,"Bioalcohol production : biochemical conversion of lignocellulosic biomass / / edited by Keith Waldron"]
[null,null,"Pubbl/distr/stampa",null,"Boca Raton, Fla., : CRC Press"]
[{"$nulls":4},"Oxford, : Woodhead Pub. Ltd., 2010"]
[null,null,"ISBN",null,"1-61344-385-4"]
[{"$nulls":4},"1-84569-961-0"]
[null,null,"Descrizione fisica",null,"1 online resource (497 p.)"]
[null,null,"Collana",null,"Woodhead Publishing series in energy ; ; no. 3"]
[null,null,"Disciplina",null,"662.88"]
[null,null,"Soggetti",null,"Cellulosic ethanol"]
[{"$nulls":4},"Biomass energy"]
[{"$nulls":4},"Lignocellulose"]
[{"$nulls":4},"Alcohols"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"pt. 1. Pretreatment and fractionation processes for lignocellulose-to-bioalcohol production -- pt. 2. Hydrolysis (saccharification) processes for lignocellulose-to-bioalcohol production -- pt. 3. Lignocellulose-to-bioalcohol fermentation and separation processes -- pt. 4. Monitoring and modelling processes in lignocellulose-to-bioalcohol production -- pt. 5. Life cycle assessment of, and multiple products from, lignocellulose-to-bioalcohol production."]
[null,null,null,"Sommario/riassunto","Bioethanol is one of the main biofuels currently used as a petroleum-substitute in transport applications. However, conflicts over food supply and land use have made its production and utilisation a controversial topic. Second generation bioalcohol production technology, based on (bio)chemical conversion of non-food lignocellulose, offers potential advantages over existing, energy-intensive bioethanol production processes. Food vs. fuel pressures may be reduced by utilising a wider range of lignocellulosic biomass feedstocks, including energy crops, cellulosic residues, and, particularly, wast"]